void InitTarget(void) {
  Report("======= Connecting to  CM4 =========");
  //JLINK_CORESIGHT_AddAP(0, CORESIGHT_AHB_AP) //0x84770001;
  //JLINK_CORESIGHT_AddAP(1, CORESIGHT_AHB_AP) //0x84770001 CM0+;
  //JLINK_CORESIGHT_AddAP(2, CORESIGHT_AHB_AP) //0x24770001 CM4; 
  CORESIGHT_IndexAHBAPToUse = 2;   

}